|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Relay type: P92x …** | | | | | | | | |
| **Software Version** | | **Hardware**  **Suffix** | **Original**  **Date of Issue** | **Description of Changes** | **S1**  **Compatibility** | **P921** | **P922** | **P923** |
| **Major** | **Minor** |
| **11** | A | HARD 5 | 06/2010 | Software changes implemented in this version (Not released for production)  - VT Supervision added,  - New combination of Fi and df/dti protections,  - Additional tAux functions,  - New 8 Boolean equations (with new operands, results usable as an operand),  - New Fail safe option,  - Addition of a bandpass filter on 59N function,  - Additional alarm inhibition,  - Addition of a new menu ORDER added,  - Digital input assignation to “Ctrl trip” and “Ctrl close” functions,  - Modification of CB operation counting,  - Addition of clock synchro. from a logic input,  - Addition of derived V0 sequence overvoltage stage,  - Addition of df/dt blocking inhibition,  - New disturbance records durations,  - New default display,  - Addition of LED reset function,  - Addition of maintenance mode of relays. | V2.14 |  |  |  |
|  | X | X |
|  |  | X |
| X | X | X |
| X | X | X |
|  | X | X |
| X | X | X |
|  | X | X |
|  | X | X |
|  | X | X |
|  | X | X |
|  | X | X |
|  | X |  |
|  | X |  |
|  | X | X |
| X | X | X |
| X | X | X |
| X | X | X |
| **11** | B | HARD 5 | 07/2010 | Software changes implemented in this version  - Several defects correction. | V2.14 |  |  |  |
| **11** | C | HARD 5 | 12/2010 | Software changes implemented in this version  - Rebranded with Schneider Electric. | V2.14 |  |  |  |
| **11** | D | HARD 5 | 12/2010 | Software changes implemented in this version  - Several defects correction. | V2.14 |  |  |  |
| **12** | A | HARD 5 | 04/2011 | Software changes implemented in this version  - Voltage balance protection added,  - General reset control added in the Order menu,  - User setting to define a Frequency cycle number before frequency fault validation added. | V2.14 |  |  |  |
|  |  | X |
|  | X | X |
|  |  | X |